# Dangerous Pi Environment Configuration
# Copy this file to /opt/dangerous-pi/.env and customize as needed

# PM3 Configuration
PM3_DEVICE=/dev/ttyACM0
PM3_TIMEOUT=30

# Session Configuration
SESSION_TIMEOUT=300

# Server Configuration
HOST=0.0.0.0
PORT=8000
VERSION=1.0.0

# Update Configuration
GITHUB_REPO=yourusername/dangerous-pi
UPDATE_CHECK_INTERVAL=3600

# Wi-Fi Configuration
WLAN_INTERFACE=wlan0
USB_WLAN_INTERFACE=wlan1

# UPS Configuration
# UPS_TYPE options: "pisugar", "i2c", "none"
UPS_TYPE=i2c
UPS_CHECK_INTERVAL=60

# I2C UPS settings (for generic fuel gauge HATs like MAX17040/MAX17048)
UPS_I2C_ADDRESS=0x36

# PiSugar UPS settings (for PiSugar 2/3 series)
UPS_PISUGAR_HOST=127.0.0.1
UPS_PISUGAR_PORT=8423

# BLE Configuration
BLE_ENABLED=true
BLE_DEVICE_NAME=DangerousPi

# Security
AUTH_ENABLED=false
HTTPS_ENABLED=false
