# Dangerous Pi Environment Configuration
# Copy this file to /opt/dangerous-pi/.env and customize as needed

# PM3 Configuration
PM3_DEVICE=/dev/ttyACM0
PM3_TIMEOUT=30

# Session Configuration
SESSION_TIMEOUT=300

# Server Configuration
HOST=0.0.0.0
PORT=8000
VERSION=1.0.0

# Update Configuration
GITHUB_REPO=yourusername/dangerous-pi
UPDATE_CHECK_INTERVAL=3600

# Wi-Fi Configuration
WLAN_INTERFACE=wlan0
USB_WLAN_INTERFACE=wlan1

# UPS Configuration
# UPS_TYPE options: "pisugar", "i2c", "none"
UPS_TYPE=i2c
UPS_CHECK_INTERVAL=60

# I2C UPS settings (for generic fuel gauge HATs like MAX17040/MAX17048)
UPS_I2C_ADDRESS=0x36

# PiSugar UPS settings (for PiSugar 2/3 series)
UPS_PISUGAR_HOST=127.0.0.1
UPS_PISUGAR_PORT=8423

# BLE Configuration
BLE_ENABLED=true
BLE_DEVICE_NAME=DangerousPi

# Security
AUTH_ENABLED=false

# HTTPS Configuration
# Set HTTPS_ENABLED=true to enable HTTPS with self-signed certificates
# On first boot with HTTPS enabled, a certificate will be automatically generated
# The certificate is valid for 10 years and covers:
#   - 192.168.4.1 (AP gateway IP)
#   - dangerous-pi.local (mDNS hostname)
#   - localhost
# Note: Browsers will show a security warning for self-signed certificates
# After enabling, restart services: sudo systemctl restart dangerous-pi-nginx-config nginx
HTTPS_ENABLED=false

# OS Updates
# Automatic security patches via unattended-upgrades (daily check)
# Set to false to disable automatic security updates
AUTO_SECURITY_UPDATES=true
